HDMI TX_SMIC_40_LL 1P8M
The design uses SMIC40LL 1P8M (1P8M_1TM) CMOS technology and digital core using metal 1~6. The power supply is 1.1V for analog and digital core devices and 3.3V for I/O devices.
Features
- 1. Single link HDMI source transmitter with PHY and Controller
- 2. Compliant with HDMI 1.4b specification and DVI 1.0 specification
- 3. HDCP 1.4 specification, internal HDCP keys, repeater not supported
- 4. Support 3D formats, 4Kx2K resolution and other common formats in CEA-861-D, such as 1080p@60Hz, 1080i/720p@120Hz and up to QXGA graphic display resolutions
- 5. Support True Color of 24 bits and Deep Color modes 30, 36, 48 bits
- 6. Support video input formats: 24/30/36/48 bit RGB 4:4:4, 24/30/36/48 bit YCbCr 4:4:4, 24/30/36 bit YCbCr 4:2:2；color space conversion and pixel repetition not supported
- 7. Digital audio interface support 4 I2S and one SPDIF,
- 8. Support link rate from 250Mbps to 3.4Gbps
- 9. CEC and HAVC not supported
- 10. I2C slave and APB configuration interface
- 11. 1.1V and 3.3V power supplies required
- 12. IP Core total area: X=2340um, Y=1100um, area=2.574mm^2
Benefits
- Harden Controller & PHY together
Deliverables
- 1.Datasheet
- 2.Flat Netlist (cdl)
- 3.Layout View (gds2)
- 4.Abstract View (lef)
- 5.Timing View (lib)
- 6.Behavioral Model (Verilog)
View HDMI TX_SMIC_40_LL 1P8M full description to...
- see the entire HDMI TX_SMIC_40_LL 1P8M datasheet
- get in contact with HDMI TX_SMIC_40_LL 1P8M Supplier
High Speed Interface
- Interlaken Protocol IP (High Speed Chip-To-Chip Interface)
- High Speed SPI AHB IP Core- Serial Peripheral Interface
- MIPI HSI Controller - (High-Speed Synchronous Serial Interface)
- USB based High Speed System Debug IP
- USB 2.0 Hi-Speed OTG Controller Subsystem w/AHB Interface Supporting HSIC (config. as Device only or Full Speed only)
- GiGE / Triple-speed Ethernet MAC 8-bit core with GMII/RGMII/SGMII interface @ 125MHz/12.5MHz/1.25MHz Solution