Tape, a circle, a wire 50 NP - alloy 50
International Equivalent
Relevance
The soft magnetic alloy precision 50 NP (50H) has a high magnetic permeability and saturation induction maintenance. It is used for the cores mezhdulampovyh, small power transformers, relays, chokes, components of magnetic circuits operated without bias or with a small magnetic bias at elevated induction. It is a magnetic material having 19 according to GOST 693−74 coercive force by induction up to 4 kA / m. has a high initial permeability, it is magnetized to saturation in weak fields, thanks to the balanced composition.
The percentage composition in accordance with GOST 10 994- — 74
Mechanical properties at 20 ° C 50 NP.
Legend:
Weldability:. Find the most widespread use in modern industry..
Supply
All products are certified 50 NP steel. The price is formed taking into account a product, the correct choice of which will depend on the performance and durability of the equipment. We will help you determine not only the optimum parameters of the product, but also offer the best price.