
 8-2018-4611
Results Found
(17)
Technology Name
Briefcase
Lead Researcher
Nanoparticle Coatings Based on Hydrogen Peroxide Sol-Gel Processing of Metal Oxides
(No. 2490)
Background Antimony tin oxide is one of the most widely used transparent conducting oxides, mainly because of its two chief properties: electrical conductivity and optical transparency, which are important for optoelectronic devices, such as in ...
More
Lev Ovadia
Cost Effective,Perovskite-based thin film solar cells
(No. 2870)
Background Large scale application of solar cells depends on attaining high solar radiation conversion efficiency, AND on further substantially reducing production costs. Solar cells are typically constructed of multilayer ...
More
Etgar Lioz
Vegetation Management for Railways and Critical Infrastructure by Non-Herbicidal Chemicals
(No. 4604)
Background Critical utilities and transportation infrastructure have demanding requirements to maintain high operational loads. It is essential that these sites will be free from encroaching vegetation which interferes with performance and ...
More
Sasson Yoel (Casali)
Gas Phase Superoxide Radicals for Soil Remediation
(No. 4561)
Background There are many areas contaminated soil all over the world and especially in industrialized countries. There is a constant demand for cost effective remediation solutions, in particular for Oil contamination. Existing ozone ...
More
Sasson Yoel (Casali)
Quantum Nano Materials for Photo-Catalytic Applications
(No. 3191)
Background The current commercial photo-initiators are unsuitable for radical-polymerization of adhesive coatings and 2&3D printing due to their poor water solubility, low efficiency and restricted suitability to the emerging LED ...
More
Banin Uri
Perovskite Nanoparticles for Display Applications
(No. 4290)
Vibrant, Efficient, Low-Cost Emitters: Background Perovskite nanoparticles are revolutionizing display technologies by down-converting some of the light from the blue LED backlight to narrow-band red and green components which results in ...
More
Etgar Lioz
Short Bio-Degradable Peptides as Anti-Bacterial and Anti-Biofilm Agents
(No. 3121)
Categories Biofilm, anti-biofilm, anti-biofilm peptides, antiseptic agent, disinfectant agents, antibacterial agents, antimicrobial agent, chemical disinfectants, biocides. Development Stage Pre-clinical proof of concept and initial ...
More
Hayouka Zvi
Biodegradable Hollow Capsule Packaging
(No. 8743)
Category Packaging Keywords 100% Biodegradable packaging , space filling, drop test Current development stage Experimental proof of concept Collaboration Opportunity Sponsored Research with an option to License Research Results ...
More
Nussinovitch Amos
Technology for in Situ Water Purification of LNAPL Pollution
(No. 4569)
Categories: Cleantech and Environment Technology Keywords: Water treatment, decontamination, remediation, AOP, hydrocarbons, LNAPL, Advanced Oxidation Process, oil spill, wastewater, ground and underground water Development ...
More
Sasson Yoel (Casali)
Doped Semiconductor Nanocrystals for Printed Electronics
(No. 2946)
Background Printed Electronics (PE) offers an attractive low cost alternative for the fabrication of electrical and optoelectronic devices which can be applied on large areas, and either on flexible or rigid surfaces. While metallic inks have ...
More
Banin Uried
A novel and facile method for 3D printing using ceramic Inks
(No. 4244)
Background Current 3D printing processes for ceramic 3D structures is conducted mainly by printing an object, which is composed of a ceramic powder and an organic binder, then sintering the body at a high temperature (>1000 °C). The ...
More
Magdassi Shlomo
Daika
(No. 13913)
Company Name Daika Year Company was Founded 2020 CEO Dr. Michael Layani About the Company Daika has developed a new material which is 100% natural. Although wood is one of the most loved raw materials, its ability to be shaped is limited. It’s ...
More
Magdassi Shlomo