MPQ4432-AEC1
Automotive Grade. 36V, 2.2A, Low Quiescent Current, Synchronous, Step-Down Converter, Available in Wettable Flank
Product Description
The MPQ4432 is a synchronous, step-down, switching regulator with programmable frequency (350kHz to 2.5MHz) and integrated, internal, high-side and low-side power MOSFETs. The MPQ4432 provides up to 2.2A of highly efficient output current with current mode control for fast loop response.
The wide 3.3V to 36V input range accommodates a variety of step-down applications in automotive input environments. The MPQ4432 is ideal for battery-powered applications due to its extremely low quiescent current.
The MPQ443232 is available in a QFN-16 (3mmx4mm) package.
Product Features
- Wide 3.3V to 36V Operating Input Range
- 2.2 (OCP))2.2
- Vfb (typ) (V)0.8
- Iq (typ) (mA)0.01
- PGNo
- GradeAutomotive
- PackageQFN-16 (3x4)
- Control ModeCurrent Mode
- Common FeaturesExternal Soft Start, Power Good, Synchronous Rectification
- Special FeaturesProgrammable Frequency
Log in to your account
Create New Account