36NHTYU Tube - EI702
International Equivalent
Composition
Mark 36NHTYU relates to chromium-nickel group of precision alloys resistant to corrosion, to as subgroup of precipitation hardening alloys. The composition of three major metal — nickel, iron and chromium with additions of titanium and aluminum. The proportion of 35−37% nickel, chromium — 11.5−13% titanium accounts for at 2.7−3.2%, aluminum 0.9−1.2% fraction, the residue — iron and alloying metals (Silicon, manganese).
The percentage of 10 to GOST 994−74.
Basic quality
Tensile strength = 1180−1570 MN / m2 (120−160 kgf / mm2). Modulus 19,6x10−15N / mm2 can be used in the production of elastic elements of high precision sensors, extreme operating temperature which is within the range 200−250 ° C. The alloy may be used in certain corrosive media, it has a high resistance to a variety of loads. Increased heat resistance is directly dependent on the structure of matter and the strong relationships between the atoms. Doping helps products withstand aggressive media, as by heating chromium, silicon, aluminum are formed on the surface of the protective film — oxides, protecting parts against further oxidation.
Using
Fragments of internal combustion engines, gas, steam, jet turbines, nuclear boilers. Pipe 36NHTYU resistant to corrosion in an industrial environment condensate at an elevated temperature. Suitable weakly in the loaded condition, for example, instrument, power plants that require high wear resistance.
Supply
All products are certified 36NHTYU brand. The technical documentation includes data on the chemical composition, limiting the percentage of impurities; mechanical properties of products. We can buy in bulk, any semi-finished products for large-scale productions. We also offer good conditions for retail customers. High level of service and efficiency of service are the face of our company.
Buy at the best price
In stock company «Electrovek-steel» is represented by a diverse range of iron-nickel.