INTERAPP PFA LINED FPCV FLANGED POPPET CHECK
Variant: FPCV - DN25-100, PN16, full bore, Carbon Steel body, PFA lining on body, hastelloy spring, PTFE poppet and -50oC to 180oC temperature range. Available in a Stainless body, conductive PFA and alternate springs.
AVK Series 570/42 gate valves
Variant: 570/42-003- DN450-600, PN16, resilient seated, flange drilling to AS/NZS 4087 B5 PN16 and AS 2129 Table E, ACC/CC, approved to AS/NZS 4020, gearbox, actuator and handwheel
AVK Series 570/92 gate valves
Variant: 570/92-003, DN450-600, PN16, resilient seated, flange drilling to AS/NZS 4087 B5 PN16 and AS 2129 Table E, Approved to AS/NZS 4020, ACC/CC, gearbox, actuator and handwheel
AVK series 57/80 gate valve
Variant: 57/80 - DN80-300, PN25, resilient seated, flange drilling to ANSI 150# or Table F, clockwise close and cap operator. Available with handwheel. Larger sizes available upon request.
AVK series 570 gate valves
Variant: 570 - DN50-400, PN16, resilient seated, flange drilling to AS 4087 B5 PN16 and AS 2129 T/E. 570/90 for Key Cap, 570/98 for Handwheel and 570/92 for ISO Mount. Available with clockwise or anti-clockwise close and Electric Actuation. .
AVK series 57/46 & 57/86 gate valves
Variant: 57/46 & 57/86 - DN50-300, PN16 & PN25, resilient seated and OS&Y. Dimensions to AS 2638.2, clockwise close and AS 4087 B5 PN16 drilling. 57/46 for PN16 and 57/86 for PN25. Optional extras include Table E drilling.
AVK series 55/74 gate valve
Variant: 55/74 - DN450-600, PN16, resilient seated, AS 4087 B5 drilling and AS 2638.2 approved. Available with clockwise or anti-clockwise close and Electric Actuation.
AVK series 55/5x & 54/3x gate valves
Variant: 54/5X & 54/3X - DN700-1200, PN16, large metal seated gate valve, flange drilling to AS 4087 with gearbox or Electric Actuation. Available with bypass (refer to series 54/5X) and without bypass (refer to series 54/3X).
UL & FM approved fire products
Variant: N/A - UL & FM approved valves. Range includes, gate valves flanged, gate valves roll groove, butterfly valves roll groove, butterfly valves double flanged, lugged and wafer pattern, check valves flanged, check valve role groove.
Gate valve rising stem
Variant: N/A - DN15-1200, Carbon or Stainless Steel construction, stellite seats, class 150-2500#, flanged connection and rising or non-rising spindle. Socket weld and threaded connections available.
Globe valve
Variant: N/A - DN15-1200, Carbon or Stainless Steel construction, stellite seats, class 150-2500# and flanged connection. Optional extras include socket weld and threaded connections, pressure seal bonnet and Y-pattern.