One-M2 Video Conference Box
One-M2 is the latest Android video conference endpoint that integrates 4k camera, microphone array and speaker as one device. It supports 1080P high-deﬁnition video conferencing, dual-screen display, electronic whiteboard, desktop sharing, remote assistance, etc., making oﬃce collaboration more convenient and eﬃcient. All-in-one design, it needs simplest cable connections and enables ﬂexible installations.
Product Features
All-in-one design
Connects via HDMI to simplify your meeting setup
Quality video experience
90° FOV camera with 15° ﬂexible tilt, make everyone clearly presented in the view. Support up to 1080p@30fps video conferencing
Premium audio performance
Built-in hi-ﬁ full-band speaker that highly reproduce human voice. The 3 omnidirectional microphone arrays supports AGC, AEC, ANS algorithms with voice pick-up range up to 5 meters, allow every participant to hear and be heard clearly.
Support dual screen display
Two monitors connected at the same time, one for video screen, the other for content sharing, to make the video collaboration more professional and eﬃcient
Works with most video collaboration apps
Based on Android system, it is compatible with most of Android video collaboration apps, including the ones that you already use.
Multiple mounting options
Flexibly to mount One-M2 wherever it works best-on the top of TV, wall, or camera stand-for the best possible huddle room experience.
Product Specifications
System Conﬁguration:
l Operating System: Android 9.0
l CPU: Corte-A72+Cortex-A53
l RAM: 4GB, ROM: 16GB
l Indicator: Loop rainbow light band; Support customization based on software
l Bluetooth 5.0
l 10M/100M/1000Mbps Ethernet
l Wi-Fi: 2.4G/5G Dual-Band, Triple antenna
Video Features:
l Support 1080p@30fps Full HD Video
l Support 1080P@30fps Projection Screen
l Hardware encoder H.264
l Hardware decoder H.264, H.265, VP8, VP9
Video Camera:
l 4K UltraHD Camera
l 90°FOV
l Manual Up and Down 15° Adjustable
Microphone Array:
l Voice pick up range up to 5 meters
l Acoustic echo cancellation
l Auto Gain Control Automatic noise suppression
Physical Interface:
l 1 x Security lock slot
l 1 x Line in/Line out
l 1 x Power Socket
l 1 x RJ45 Ethernet port
l 1 x RJ45 for Expansion Microphone
l 2 x HDMI Out
l 1 x USB
l 1 x Reset Hole
Other Specification:
l Product size: 400mm x 87mm x 87mm
l Power supply: DC12V@2A
l Warranty: 12 Months
l Application: Enterprises Video Conferencing, Business Negotiations, remote education and training, Telemedicine and remote medical consultations.
l Operating temperature: 0~40°C
l Relative humidity: 5~95%, noncondensing
l Storage temperature: -10~70°C
Typical Application
