GEOCOIR®/DeKowe® Biodegradeable Geotextiles
GEOCOIR®/DeKowe® biodegradable geotextiles are used for slope stabilization and protection of stream banks, shorelines and wetlands. They are made from exceptionally high strength woven coir fiber twine.
GEOCOIR®/DeKowe® biodegradable geotextiles are available in 3 standard weights, 400, 700 and 900 grams/sq meter and the unique 2307 fencing system.
GEOCOIR®/DeKowe® biodegradable geotextiles hold seed and plant materials in place as the vegetation takes hold. As soon as they accomplish their function, (up to 10 years depending upon application) GEOCOIR®/DeKowe® biodegradable geotextiles decompose and fit into the natural ecological cycle, leaving a flourishing, healthy natural vegetative barrier against further erosion problems.
Dekowe 700 is approved for use as a WI DOT class 2C erosion mat.
Antiwash®/Geojute® Biodegradeable Geotextiles
ANTI-WASH®/GEOJUTE® is the answer to short term soil stabilization problems. Made from natural fiber jute, un-dyed and unbleached, it is totally biodegradable within two years. ANTI-WASH®/GEOJUTE® is excellent for landscaping as it controls erosion in new plantings. Plantings can be made after installation is complete.
100% jute blanket is approved for use as a WI DOT class 2A erosion mat.