How do I reset network setting?
Follow the instructions below:
For RJ-3050/3050Ai
- Press and hold the
(Power) button to turn the printer off.
- Press and hold the
(Feed) button and the
(Power) button for about 3 seconds. The POWER, Wi-Fi® and Bluetooth® indicators start blinking (POWER: in orange; Wi-Fi and Bluetooth: in blue).
- While pressing the
(Power) button, press the
(Feed) button once.
- Release the
(Power) button.
For RJ-3150/3150Ai
- Press the Menu, Up or Down arrow button to select the Administration menu, and then press the OK button.
- Select Reset > Network Reset > Reset using the Up or Down arrow button, and then press the OK button.
If your question was not answered, have you checked other FAQs?
Have you checked manuals?
If you need further assistance, please contact Brother customer service:
Content Feedback
To help us improve our support, please provide your feedback below.