Master level technician - Apple MacBook Pro and iMac repairs.
Expert level technician - iProduct repairs.
IT Amazing! located in Santa Cruz.
Absolvierte Anleitungen
Fragen
- Maximum Fingerprint Limit Reached after Top-Case ReplacementI have this Macbook Pro 15 inch Touch-bar 2017, I swapped the top case to fix my keyboard, all features working perfect when ...
-...
Antworten
- Hat geantwortet auf: iPhone 6s Black screenIt sounds like the screen is defective. You could try reseating that LCD Assembly you purchased, just in case it isn’t fully seated onto it’s connector on the board. Edit: Can you return said screen for another one?
- Hat geantwortet auf: MacBook Air beach balling frequently. :)
- Hat geantwortet auf:
- Hat geantwortet auf: Tin can audio from replacement screen iPhone 6sIn.
- Hat geantwortet auf: Sata cable problem for MBP 15 MID2012There are two different cable versions of this Cable: 821-1492-01 (was recommended) 821-1492-A (what you have) They Are Backwards-Compatible, yes. You aren't losing anything by using your A version.
- Hat geantwortet auf: My new digitizer's bottom half of the screen is not registering touch.If you can reseat that digitizer connector by pulling it out and putting it back in, you'd be surprised how many problems that solves. :) It's worth noting, that if your iPad had any power at time of replacement, erratic behavior can occur. I recommend you hold both the Sleep/Wake and Home buttons for at least ten seconds, until you see the Apple logo, before considering the digitizer defective.
- Hat geantwortet auf: Track pad and Keyboard stopped working except power buttonDan's Answer to a similar problem in 2014: Give him credit if it works. The keyboard/track pad ribbon cable from the top case is not seated correctly into the logic board connector (or damaged). Something was spilled into the keyboard and it took a bit of time to damage the connections. The last possibility is the battery has swelled pressing from under the keyboard causing it to fail. To test for the battery problem, put your laptop into a plastic bag making sure to pull out as much air out as you can. Place the laptop into your refrigerator for about an 2 hours to drop its temp. Take it out and quickly turn it on, see if the keyboard and track pad are working. If they are the issue is the battery pressing on the top case from below. If your upto it pop off the bottom cover to inspect the ribbon cable to see if its correctly seated. Otherwise you'll likely need a new top case as the keyboard is part of it.
- Hat geantwortet auf: How do I fix thisThe most affordable and reliable Option would be to utilize Apple's Out of Warranty Repair Service! It would cost a flat $150. I can't even buy the screen for that much, not including the 100 labor i'd charge to fix it. Here's a list of Apple's Out of Warranty Costs: In summary: To the Apple Store, and Beyond!
- Hat geantwortet auf: Verticlal White Stripes on MacBook 2009 LCDIt could be the LVDS cable or the LCD itself. Let's try something: Open the Macbook into an Obtuse position (wider than 90 degrees open.) Do it a few times; Do any of the white lines change formation or position? If they DO, the LVDS Cable is more likely the problem. If this technique does NOT produce any change in the distortions, then the LCD itself is more likely to blame. Best Solutions: EZ Mode - Buy an LCD Assembly! Here's a link to a 13 inch 2009 LCD Assembly. See our handy guide on how to install said LCD Assembly, it's much easier than the other options. It's about $100 total!...
- Hat geantwortet auf: Laptop won't boot upIf you're running Windows 8 or 10, you will have to trigger a refresh to solve the problem. I believe the answer key was F11. Top of F11 once per second the moment you turn your computer on, if that doesn't work after 15 seconds so, pull down your power button for six seconds until the computer turns off, and try again. If you fail this three times it will trigger a Windows 8 or Windows 10 automatic repair. From there, click on troubleshooting, and click refresh your PC - warning if you hit reset your PC you will lose everything, use the refresh feature specifically. If you're running Windows 7, repeat this process but instead of tapping F11, tap if instead. Try logging in with that code or password again, And let's see if it does any better.
Tread very, very carefully with that LCD panel.
One must consider, the USP based card adapter is like five dollars.
When I tell customers this, they usually get that instead of paying me $100 plus parts to repair it
If you can replace the airport card, try to replace the daughterboard that it resides in while you are at it.
Tedious as heck, but better than plopping a USB camera on the top or on the side. :-).
Go slow, and take your time. Easy as long as you do not rush it.
Do everything in your power to avoid touching the inside of the glass with your fingers, or the LCD. Please give me his fingerprints is like washing and oiled animal with water :)
Seite 1 von 2
Weiter